**PI – Configure Static IP on ETH0**

This is a quick guide on how to set a static IP on the network card

From the **command prompt**, type:

**sudo bash** and press enter

**nano /etc/network/interfaces** and press **enter**

Change the following entry from:  
iface eth0 inet dhcp

Change it to: **iface eth0 inet static  
address 192.168.1.10  
netmask 255.255.255.0  
gateway 192.168.1.1  
network 192.168.1.0  
broadcast 192.168.1.255**

Press **CTRL** and **O** at the same time to save

Press **CTRL** and **X** together to exit

**Reboot**